# Telephone Entry System Remote Programmer for Android

[![License](https://img.shields.io/badge/license-Apache%20License%202.0-blue.svg)](https://opensource.org/licenses/Apache-2.0)
[![Build Status](https://travis-ci.org/ethauvin/TESRemoteProgrammer.svg?branch=master)](https://travis-ci.org/ethauvin/TESRemoteProgrammer)
[![Known Vulnerabilities](https://snyk.io/test/github/ethauvin/tesremoteprogrammer/badge.svg?targetFile=app%2Fbuild.gradle)](https://snyk.io/test/github/ethauvin/tesremoteprogrammer?targetFile=app%2Fbuild.gradle)
[![CircleCI](https://circleci.com/gh/ethauvin/TESRemoteProgrammer/tree/master.svg?style=shield)](https://circleci.com/gh/ethauvin/TESRemoteProgrammer/tree/master)
[![License](https://img.shields.io/badge/android-Privacy%20Policy-orange.svg)](https://thauv.in/apps-privacy)


[![TES Remote Programmer](https://github.com/ethauvin/TESRemoteProgrammer/raw/master/images/github_graphic.png)](httpd://mobile.thauvin.net/android/)

Program your Telephone Entry System remotely (off-site) using your phone.

Most Telephone Entry Systems can be programmed from the front keypad or remotely from an off-premise location using any touch-tone phone. TES Remote Programmer streamlines the often cumbersome remote programming process by providing data entry screens and automated dial-in options.

### DoorKing (DKS) & Linear

By default, TES Remote Programmer is configured to work with the [DoorKing 1802, 1802-EPD, 1803, 1808, 1810 and 1819](http://www.doorking.com/telephone/) as well as the [Linear AE-100 and AE-500](http://www.linearproaccess.com/access-controls/telephone-entry-systems/) systems, additional [configurations](#configurations) can be created for most systems supporting remote programming.

### Directory Code

Please note that all default configurations are set for 3-digits directory code length. If your system is setup differently, you will need to modify the [default configuration](app/src/main/res/raw/) and re-import it. Look for all `Directory Code` fields and modify their `size` attributes accordingly.

## Usage

![Main Activity](images/screenshots/main_activity_framed_small.png)

In the main activity screen enter the entry system's phone number and master code, then select one the programming options.

![Programming Activity](images/screenshots/add_phone_number_framed_small.png) ![Programming Activity](images/screenshots/set_time_clock_framed_small.png)

In the programming activity screens fill out the fields and click the ![Dial](images/call_fab.png) floating button (if available) to dial the programming in or the ![Dial](images/dialpad_fab.png) floating button to scroll through the manual (keypad) steps.

## Configurations

![Configurations](images/screenshots/configurations_framed_small.png)

To switch configuration, choose `Configurations` under the toolbar menu and select the desired configuration.

To import a new configuration, select `Import` in the _Configurations_ dialog.

### New Configurations

Custom configurations can be created using [JSON](http://www.json.org/).

[View Examples](app/src/main/res/raw/)

#### Parameters

Parameters define the configuration's global settings.

```json
"params": {
  "name": "DKS 1802-EPD",
  "type": "dks",
  "ack": "*",
  "alt": "#",
  "end": "0 + #",
  "size": 4
}
```

| Property | Description                                                                                       | Required |
|:---------|:--------------------------------------------------------------------------------------------------|:---------|
|`name`    | The name of the configuration.                                                                    | Yes      |
|`type`    | The system's type, either `dks` or `linear`. See note below.                                      | Yes      |
|`ack`     | The key used to acknowledge or terminate programming steps. Most systems use the `*` or `#` keys. | Yes      |
|`alt`     | They key used to in place of numbers when applicable. DKS systems use the `#` key                 | No       |
|`begin`   | The begin programming manual sequence. (e.g. Linear uses `0` and `2` pressed together)            | No       |
|`end`     | The end programming manual sequence. (e.g. DSK uses `0` and `#` pressed together.)                | No       |
|`size`    | The size (number of digits) of the master code. Most systems use 4 or 6.                          | Yes      |

The `type` is used to determine how letters are converted to digits in alphanumeric (`alpha`) [fields](#fields), both DKS and Linear use different methodologies. It is also used to allow numeric values with leading zeros (e.g. `001`) on DKS systems.

### Options

Options define the data used to create programming activity screens in the app.

For example, the system's manual lists the steps to _Programming 7-digit Phone Numbers_ as:

1. Press *01 and enter Master Code.
2. Enter a Directory Code then press *.
3. Enter a 7-digit Phone Number then press *. If the number is less than 7-digits, enter # in the empty spaces.
4. Press 0# TOGETHER when finished.

which would translate into:

![Options](images/options_example.png)

```json
"opts": [
  {
    "title": "Add 7-digit Phone Number",
    "fields": [
      {
        "hint": "Directory Code",
        "size": 3
      },
      {
        "hint": "Phone Number",
        "size": 7,
        "alt": true
      }
    ],
    "dtmf": "*01[MASTER],[FIELD:1]*,[FIELD:2]*"
  }
]
```

Step 4 is configured in the `end` [parameter](#parameters) since it only applies to manual/keypad programming.

| Property | Description                                                                                       |
|:---------|:--------------------------------------------------------------------------------------------------|
|`title`   | The title of the option.                                                                          |
|`fields`  | See [Fields](#fields)                                                                             |
|`dtmf`    | See [DTMF](#dtmf)                                                                                 |
|`nodial`  | Indicate that remote programming is not available. Steps must be executed manually at the keypad. |
|`nosteps` | Indicate that manual/keypad steps are not available. Programming must be executed remotely.       |

All are required, except `nodial` and `nosteps` which are mutually exclusive.

#### Fields

```json
"fields": [
  {
    "hint": "Directory Code",
    "size": 3
  },
  {
    "hint": "Phone Number",
    "size": 7,
    "alt": true
  }
]
```

Fields represent the data entry text fields on option screens.

| Property | Description                                                                                                                                             | Required |
|:---------|:--------------------------------------------------------------------------------------------------------------------------------------------------------|:---------|
|`hint`    | Set the hint/label of the field.                                                                                                                        | Yes      |
|`size`    | Set the size of the field.                                                                                                                              | Yes      |
|`minSize` | Set the minimum size of the field. If set, `size` is the maximum size of the field.                                                                     | No       |
|`alpha`   | Set to `true` for alphanumeric fields.                                                                                                                  | No       |
|`min`     | Set the minimum value of a numeric field.                                                                                                               | No       |
|`max`     | Set the maximum value of a numeric field.                                                                                                               | No       |
|`digits`  | Set digits that are allowed. (e.g. DKS uses `1234567` for days of the week: Sun=1... Sat=7)                                                             | No       |
|`alt`     | Set to `true` if the field accepts the `alt` [parameter](#parameters) value in place of a digit.                                                        | No       |
|`zeros`   | Set to `true` by default when the `type` [parameter](#parameters) is `dks`. Allows numeric values with leading zeros (e.g. `001`), based on the `size`. | No       |


#### DTMF

```json
"dtmf": "*01[MASTER],[FIELD:1]*,[FIELD:2]*"
```

DTMF represent the dialing sequence for the programming steps. A comma (`,`) should be used to specify a pause in the dialing sequence.

The following markers will be substituted by their actual values upon dialing.

| Marker     | Description                                                                               |
|:-----------|:------------------------------------------------------------------------------------------|
|`[MASTER]`  | Substituted with the Master Code                                                          |
|`[FIELD:X]` | Substituted with the field's value, where X is the field number in the array.             |
|`'Foo bar'` | Displays the enclosed text as a manual step. The `nodial` [option](#options) must be set. |

#### Validation

Imported configurations will be validated. While the validation is not perfect, it should be good enough to spot most syntax errors.

Please sure to use a JSON editor to make creating configurations a whole lot easier.

When in doubt be sure to look at the [default configurations](app/src/main/res/raw/).
